***SCORING GUIDELINES FOR PRACTICAL EXAM***

***MASONRY***

* ALWAYS CHECK YOUR HEIGHT FROM THE SAME SPOT (SAME CORNER) EACH TIME. YOUR GRADE WILL BE BASED ON THE HEIGHT FROM THE CORNER YOU START FROM.
* ALWAYS USE THE SAME SET OF LEVELS. YOUR JUDGE WILL GRADE YOUR PROJECT WITH YOUR LEVEL.
* BLOCK USES A SCALE “2” AND MODULAR BRICK ARE SCALE “6”, SO (3) BRICK SHOULD EQUAL THE HEIGHT OF (1) BLOCK
* YOUR JUDGE WILL TAKE AN AVERAGE OF (8) PLUMB POINTS FOR GRADING
* YOUR GRADE FOR LEVEL WILL BE DETERMINED BY THE LAST COURSE COMPLETED
* BE SURE TO FILL ALL JOINTS BUT DON’T TOOL THE JOINTS UNTIL THEY ARE READY……THAT WILL HELP WITH THE NEATNESS.
* THE RANGE GRADE WILL BE DETERMINED BY CHECKING THE RANGE OF THE BLOCK DIAGONALLY AS WELL AS THE BRICK DIAGONALLY. UP TO 5 POINTS EACH SIDE TOTALLING 10 POSSIBLE
* YOU HAVE PLENTY OF TIME SO DO NOT RUSH…***QUALITY IS BETTER THAN QUANTITY.***  USE YOU TIME EFFECTIVELY-THIS COUNTS FOR 20%
* GOOD LUCK AND FOLLOW ALL SAFETY REQUIREMENTS